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Hero Slogan XENONS Dafey 2 is New-Gen 2 DTF System — Built on User Insights, Leading the Next Industry Upgrade User-Driven Innovation. XENONS New Gen 2 industrial DTF Powers Your Factory Upgrade.
Product Overview
The XENONS DTF D6006 Plus Dafey Gen2 is the brand-new upgraded 6-head high-speed DTF printing solution launched in 2026. This all-in-one industrial 24” DTF printer integrated with powder shaker and curing system is engineered exclusively for high-volume garment heat transfer production. It is equipped with 6 new Epson I3200 A1/A2 industrial printheads, supporting a maximum media width of 600mm.
It is ideal for factories manufacturing heat transfers for T-shirts, hoodies, canvas bags, denim, labels and custom textile goods. Designed for continuous bulk production rather than entry-level small-scale DTF printing, it is the perfect workhorse for growing print businesses looking to scale output and boost profit margins.
Core Technical Highlights
· Printheads: 6 × New Epson I3200 A1/A2 industrial printheads
· Print Width: 24 inch / 600 mm
· Max Printing Speed: Up to 60 ㎡/h
· Ink Configuration: 4C + 3W (4 colors + 3 white inks)
· Core Performance: Outstanding stability, ultra-high speed, premium print quality
· Labor & time saving: Batch printing supported, one-touch operation for powder shaker
· Cleaner workshop environment: Built-in purifier to prevent powder leakage
· Global IoT-enabled printer fleet management system
· Compatible with efficient MES job management system to cut labor cost for production management
Why Choose XENONS D6006 Plus Dafey Gen2?
✅ Massive Production Capacity 6 printheads paired with 4C+3W ink layout delivers up to 60 sqm/h output, greatly boosting daily throughput for large garment printing orders.
✅ Reliable Industrial Grade Performance Built for non-stop continuous production. The Epson I3200 A1/A2 printheads deliver consistent ink laydown for sharp, vibrant transfers across full roll jobs, minimizing waste and rework.
✅ One-Powder-Shaker Integrated System All-in-one design combining printing, powder application, shaking and curing. One-touch powder shaker control cuts manual operations and simplifies workflow for your operators.
✅ Clean & Eco-Friendly Workshop The integrated purification system captures excess powder, stopping powder spillage and keeping your factory floor clean, reducing health risks and meeting modern factory environmental standards.
✅ Smart Factory Ready Built-in global IoT remote monitoring allows you to track machine status, production data and fault alerts from anywhere. Native compatibility with MES production management software reduces manual work for order scheduling and production statistics.
Ideal For
· Medium & large-scale garment printing factories
· DTF transfer film suppliers
· Manufacturers producing large volumes of T-shirts, hoodies, bags, labels and textile transfer films
· Factories requiring continuous production with automatic powder shaking and curing units
Not Suitable For
· Home users
· Micro startups with very low daily order volume
· Buyers without stable power supply, humidity control or trained operating staff
Technical Specification Table
表格
	Item
	Specification

	Model
	XENONS DTF D6006 Plus Dafey Gen2

	Printheads
	6 × Epson I3200 A1/A2 industrial printheads

	Max Print Width
	24 inch (600 mm)

	Max Print Speed
	Up to 60 ㎡/h

	Ink Setup
	4C +3W (CMYK + 3 White)

	System
	Integrated printer + powder shaker + curing & purification system

	Smart Functions
	IoT remote fleet management, MES compatible


Application Industries & Materials
Our DTF system works perfectly on most textiles, including cotton, polyester, cotton blends, denim, canvas, nylon, and many more. Common products: T-shirts, hoodies, sweatshirts, workwear, canvas bags, caps, custom labels, fashion accessories, promotional merchandise.
After-sales & Support
XENONS provides global technical support, remote online troubleshooting, machine firmware updates, operator training guides and spare parts supply. Our IoT system enables fast remote diagnosis, minimizing downtime for your production line.
Brand Promise
XENONS designs industrial DTF equipment based on real-world feedback from printing factory owners. We focus on practical, production-proven upgrades rather than empty specifications. D6006 Plus Dafey Gen2 is the next-generation workhorse for high-volume textile transfer printing, helping your factory increase output, reduce operational cost and stay competitive in the global apparel printing market.
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